CJ5 ('55 - '71) & M38A1 ('51 - '71) Windshield width 59", round fender Jeep, one piece windshield, no factory door hinges, windshield retainer welded on vehicle, windshield at 90° angle to hood. 

CJ3B ('53 - '64) Windshield height 22 1/2", hood height 10 1/2" (fender to top of hood), one piece windshield, has tailgate, bottom mounted windshield wipers, side mounted tire carrier (factory). 

CJ3A & M38 ('48 - '53) Windshield height 27", flat fenders, one piece windshield, vent in middle of windshield (factory), bottom mounted windshield wipers, hood height 6" (fender to top of hood). 

CJ2A & M38 ('46 - '49) Windshield height 25", flat fenders, split windshield, has tailgate, top mounted windshield wipers, side mounted spare tire (factory), hood height 6" (fender to top of hood). 

MB ('41 - '45) Windshield height 23", flat fenders, split windshield, no tailgate, recessed headlights top mounted windshield wipers, rear mounted spare tire (factory), hood height 6" (fender to top of hood).